Settings > Extended:

Show VU Meter until recording:
Shows the stereo VU meter in the VoiceTrack tab during recording.
Note: The VU meter uses a paint box (not a system progress bar) to avoid
screen reader beeping noises from accessibility events. It can be disabled here
if still causing issues with your screen reader.

Show information about current On-Air track:
Activates the On-Air status display at the top of the main window
(requires RadioBOSS API). When disabled, the entire top area remains hidden.

Select On-Air tab while available on app startup:
If the On-Air list can be loaded on startup, the OnAir tab is automatically
selected in the left tab window.

Use Enter key for changing directories directly:
When active, pressing Enter in the FTP list navigates directly into the selected
directory instead of opening the dropdown menu.

Language:
Dropdown field to select the display language.
Available: German, English, French, Spanish, Turkish.
Change takes effect immediately after saving.

Local RadioBOSS Host / User / Password:
Optional connection settings for a second (local) RadioBOSS instance.
When configured, the 'Local' checkbox appears next to the On-Air status display.
Used for switching between an external broadcast server and a local studio system.
Progress bar note: When the relay is disabled, the progress bar in the On-Air panel
spans the full width; when active or waiting, it shares the space with the relay status text.
